**PRICE ATTRIBUTE RESPONSES**

**SCHEDULE OF PRICES** (for completion)

|  |
| --- |
|  |
| Item | Description | Unit | Quantity | Rate | Amount |
| **1** | **Preliminary and General** |
| 1.1 | Preliminary and general - Establishment | LS | 1 |  |  |
| 2 | **Materials as per Bill of Quantity** |
| 2.1 | Supply and delivery to site of the materials listed in the Bill of Quantity | LS | 1 |  |  |
| 3 | **Construction**  |
| 3.1 | Fence construction, including security, labour and all other aspects of the project | LS | 1 |  |  |
| **TOTAL**  | $ |

**Tenderer’s signature**: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

**Tenderer’s role/position:** ­­­­­­­­­­­\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

**Date:**  \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

**BILL OF QUANTITIES** (for completion)

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **MATERIAL LIST**  | **QUANTITY**  | **UNIT**  | **RATE**  | **SUB TOTAL**  |
| 50 mm dia galv. Posts  | 94 | 6M lths  |  |  |
| 75mm dia galv.corner Posts  | 10 | 6M lths  |  |  |
| 40mm dia galv. bracings  | 5 | 6M lths  |  |  |
| 1.2m chainlink  | 45 | 15M per roll  |  |  |
| Barbed wire  | 6 | 500m per roll  |  |  |
| Dricon-Handicrete bags  | 281 | 25kg / bag  |  |  |
| Post cap  |  |  |  |
|  | 281 |  |  |
|  |  |  |  |
| Metal grinding discs  | 10 | pcs  |  |  |
| Metal cutting discs  | 10 | pcs  |  |  |
| Wire ties  | 10 | kg  |  |  |
| 2.5 welding rods  | 5 | pckts  |  |  |
| Shovels  | 2 | pc  |  |  |
| Juo sipeti  | 3 | pc  |  |  |
| Huo langa  | 2 | pc  |  |  |
| Hele pelu  | 3 | pc  |  |  |
| Chainsaw  | 2 | pc  |  |  |
| Machine oil  | 5 | ltrs  |  |  |
| Petrol fuel  | 20 | ltrs  |  |  |
| Spark plugs  | 3 | pc  |  |  |
| Tool kit  | 1 | box  |  |  |
| Fence tensioner  | 2 | pc  |  |  |
| Jack hammer drill  | 2 | pc  |  |  |
| Generator 1  |  |
|  |  |
| *Material cost*  |  |
|  |  |
| *4 liters of water for each post, this could be 1124 liters of water needed. So, the contractor must make sure it has a 1124-liter tank* |  |